# Chapter 1: Tour of WICED WiFi

## Objective

After completing chapter 1 you should understand a top level view of all of the components of the WICED ecosystem including the chips, modules, software, documentation, support infrastructure and development kits. You should have WICED installed and working on your computer and should understand how to program an existing project into a kit.

## Time: 2 Hours

## Fundamentals


### Tour of WICED WiFi SDK

#### Eclipse

The WICED WiFi SDK is based on Eclipse. Currently, the IDE is different for WiFi and Bluetooth although both are based on Eclipse. We will be using the WiFi SDK version 3.7.0-3. However, starting with WICED Studio 4.0, there will be a single IDE for both WiFi and Bluetooth.

The Eclipse software is by default installed in *C:\Program Files (x86)\WICED*, but the actual SDK workspace will be located in *C:\Users\<UserName>\My Documents\WICED\WICED-SDK-<version>\WICED-SDK*. This is where you will typically create your projects. Note that a new set of SDK files is created for each version of the SDK so if you install a newer version your projects will still be available in the old location – you have to copy them over manually if you want to access them in the new SDK.

Once installed, the SDK will show up in Windows under Start > All Programs > Broadcom > WICED IDE. When you first open the program, you will see a window that looks like this:



The major windows are:


1. File Editor
2. Project Explorer
3. Make Target
4. Console
5. Help

If you close a window unintentionally, you can restore the original set of windows using the following procedure:

1. Select Window > Reset Perspective
   1. Note: the perspective shown is *C/C++.* You can open other perspectives by clicking the icon near the top right corner of the screen or by using Window > Open perspective.
2. Click on the Make Target tab in the upper right window
3. Click on the Console tab in the bottom window
4. Select Window > Show View > Other… > Help > Help
5. Drag the Help tab to the right to dock it to the side of the Output area

#### Project Explorer

If you expand WICED-SDK from the Project Explorer window you will see the following:



Note: you can access these files from Windows explorer at: *C:\Users\<UserName>\My Documents\WICED\WICED-SDK-<version>\WICED-SDK*

The README.txt file provides basic information about the SDK. This file is open by default in the editor window when the SDK is first opened. Other folders of interest in the Project Explorer are:


##### Apps

The apps folder is where the projects reside. The SDK includes a wealth of example projects. These are broken into categories by folder name. A few of the useful ones are:

1. Snip: These are short examples that typically demonstrate one feature such as how to use GPIOs, or how to scan for WiFi networks.
   1. snip.gpio demonstrates reading buttons and blinking LEDs.
   2. snip.scan will scan for WiFi access points every 5 seconds and will display the results to a terminal window.
2. Demo: These are more complex, complete demonstrations such as a Bluetooth to WiFi Bridge, or temperate control and report application.
3. Test: These are test and utility programs such as a console that allows you to scan for and connect to WiFi access points.
   1. test.console will provide a console application on a terminal window. Type “help” in the console for a list of all supported commands.

##### Doc

The doc folder contains various documentation. Of particular interest is the API.html file which documents all of the WICED API functions. It is usually easier to use that file if you open it in a web browser of your choice rather than from inside the SDK. The first window you will see when you open the API.html file is shown below.



##### Platforms

The platforms folder contains information on kit (i.e. hardware platform). These files are necessary in order to program a given project into the hardware you are using. That is, the platform name provided in the make target must match one of the platforms in the platforms folder. In our case, the kit we are using is called BCM94343W\_AVN. That isn’t installed by default so we will have to copy in the platform files before using it. You can even create platform files for custom hardware that you design. We’ll discuss the platforms folder in more detail in chapter 2.

##### Libraries

The libraries folder contains various sets of library function files. For example, there are libraries for working with file systems (in the filesystems folder) and for using U8G graphics LCDs (in the graphics folder). We will discuss the libraries folder in more detail in chapter 4.

##### Resources

The resources folder is where you store files that are required by your application. For example, if your application contains a web server, the html files for the server would be in the resources folder under *apps\https\_server*.


#### Make Target

The Make Targets are how you program and run your application. The make target will be explained in more detail in chapter 2.

### Tour of Documentation

#### In the SDK

As discussed previously, the doc folder in the SDK contains various documents such as the API guide. That folder also contains other documents such as the QSG (Quick Start Guide), how to use DCT (Device Configuration Tables), FLAC (Free Lossless Audio Compression), and OTA (Over the Air) Updates. The list of files in the doc directory is:



Each of the files in the doc folder can be accessed either from within the SDK or from Windows explorer.

#### On the Web

[www.cypress.com](http://www.cypress.com) > Design Support > WICED Software will take you to the following site (the direct link is <https://community.cypress.com/welcome>):



Clicking on WICED Wi-Fi will take you to the community page as shown below. From this page, you can download the SDK, purchase kits, search for answers, ask questions, etc.



### Tour of WiFi

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **IEEE Standard** | **Bandwidth** | **Frequency** | **Channels** | **Channel Width** | **MIMO/SISO** | **Range** |
| [802.11a](https://en.wikipedia.org/wiki/IEEE_802.11a-1999) | 54 Mbits/s | 5 GHz |  |  |  |  |
| [802.11b](https://en.wikipedia.org/wiki/IEEE_802.11b-1999) | 11 Mbits/s | 2.4 GHz |  |  |  |  |
| [802.11g](https://en.wikipedia.org/wiki/IEEE_802.11g-2003) | 54 Mbits/s | GHz |  |  |  |  |
| [802.11n](https://en.wikipedia.org/wiki/IEEE_802.11n-2009) | 600 Mbits/s | 2.4GHz / 5 GHz |  |  |  |  |
| [802.11ac](https://en.wikipedia.org/wiki/IEEE_802.11ac) |  |  |  |  |  |  |

### Tour of Chips

4343W + 43438

TBD

4390x (43907, 43903, 4390)

TBD

43362 + 43364

TBD

### Tour of Modules

### Tour of Development Kits

#### [Cypress BCM94343WWCD1\_EVB Evaluation and Development Kit](http://www.cypress.com/products/ieee-80211abgn-wlan-bluetooth-edr-usb-sdio-and-pcie)

* WiFi + BLE combo kit (BCM4343W)
* 512kB Flash, 128kB SRAM, 8Mb SPI Flash
* 2 User Buttons, 2 User LEDs
* Thermistor
* USB JTAG Programmer/Debugger

#### [Avnet BCM4343W IoT Starter Kit](http://cloudconnectkits.org/product/avnet-bcm4343w-iot-starter-kit)

* WiFi + BLE combo kit (BCM4343W)
* 512kB Flash, 128kB SRAM, 8Mb SPI Flash
* 1 User Button, 2 User LEDs
* Ambient Light Sensor
* Arduino Compatible Headers
* USB JTAG Programmer/Debugger

#### [Adafruit Feather](https://www.adafruit.com/products/3056)

* WiFi kit (BCM43362)
* 128kB Flash, 16kB SRAM, 16Mb SPI Flash
* Programmable using Arduino IDE
* USB Bootloader


#### [Electric Imp](https://www.electricimp.com/platform/)

* WiFi kit (IMP003- BCM43362, IMP005 – BCM43907)
* Programmable using imp IDE

#### [Inventek](http://www.inventeksys.com/)


ISM43362-M3G-EVB

* WiFi Kit (BCM43362)
* 2 User Buttons, 2 User LEDs
* Thermistor
* USB JTAG Programmer/Debugger

ISM43340-M4G-EVB

* WiFi & Bluetooth Combo Kit (BCM43340)
* 2 User Buttons, 2 User LEDs
* Thermistor
* USB JTAG Programmer/Debugger


ISM43341-M4G-EVB

* WiFi, Bluetooth, NFC Combo (BCM43341)
* 2 User Buttons, 2 User LEDs
* Thermistor
* USB JTAG Programmer/Debugger


ISMART Arduino Shield

* WiFi, Bluetooth, NFC Combo (BCM43362)
* Arduino stackable shield

ISM43340-L77-EVB

* WiFi & Bluetooth Combo Kit (BCM43340)
* WiFi over SDIO
* Bluetooth over UART
* Micro-SD Connector

#### [Particle](https://www.particle.io/products/hardware/photon-wifi-dev-kit) [Photon](https://www.particle.io/products/hardware/photon-wifi-dev-kit)

* WiFi kit (BCM43362)
* 1MB Flash, 128kB SRAM

#### SparkFun with Particle Photon Module

* WiFi kit (BCM43362)
* 1MB Flash, 128kB SRAM
* Arduino Compatible Headers

## Exercise(s)

### Create a forum account

1. Go to <https://community.cypress.com/welcome>
2. If you already have an account, click “Log in” from the top right corner of the page.
3. If you do not have an account, click “WICED Community” from the panel on the left and sign up for an account.
4. Once you are logged in, click the “WICED Wi-Fi” icon.
5. Click on the “Forums” button.
6. Browse the existing forum articles or search for a particular topic that interests you.

### Open the documentation

1. Open the API.html document from the WICED SDK doc directory.